{"text_format":"2","workbook":"xls","n_sheets":4,"sheets":["1 - Overview","2 - SPA525G Speed Dials","3 - Sidecar SPA500S","4 - Dial Outside Line"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1 - Overview","index":0,"n_rows":9,"n_cols":1,"rows_kept":9,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Hello. This excel sheet has 4 tabs at the bottom. Currently you are on Tab-1, the overview tab. "]
[]
["Tab #2 is a worksheet that will create the syntax you need, that goes into your phone, in order to create Speed Dial buttons from unused ‘Line’ buttons on your Cisco Phone. The worksheet will let you enter the extension number you want as a speed dial, and the text you want to ‘Name’ that speed dial. Then you click the purple button and the sheet will produce the syntax you need to ‘copy-n-paste’ into your phone."]
[]
["Tab #3 does pretty much the same thing as Tab #2, except that this is to be used with the SPA-500 series ‘Sidecars’. You will see the left most two columns are numbered 1 through 32. On each box there is a ‘top’ line and a ‘bottom’ line. On the ‘top’ line you enter the extension number you want as a speed dial. On the ‘bottom’ line you enter the speed dial description. When you are done, scroll down until you see the light-blue box. When you click the ‘Calculate’ button, the sheet will then produce the syntax you will need to ‘copy-n-paste’ into each button on your Sidecar in order to use your Sidecar for speed dialing. This ‘syntax’ will appear on the far right side, in column ‘H’."]
[]
["On Tab #3, you will notice there is also a set of boxes in the ‘middle’ of the sheet. This ‘middle’ section automatically produces the text you designated for each speed dial button as you created them. This ‘middle’ sheet is PRINTABLE. When you ‘print’ this sheet, you will see only this ‘middle’ section. This is for users of the 500-S series Sidecar. Printing this sheet will now give a sheet that you can cut out and place into the center of your Sidecar so you know what buttons are associated with what speed dials."]
[]
["Tab #4 is for use on the Cisco SPA-525, where users have linked their cellphones to line button #5 via bluetooth. On this tab, you can enter a ‘phone number’ and a ‘text name’ and then click the red button. The sheet will now calculate the syntax you will need to ‘copy-n-paste’ into any of your speed-dial buttons on either your Cisco SPA-525 or on your SPA-500 series Sidecar. After you program the desired speed dial button and save it, once you press that specific speed dial on your device, your Cisco phone will then pick-up line #5 on your Cisco phone, and pair with your cellphone to make that call. You talk via your Cisco phone, but the call is actually being made on your cellphone. This is just the same as using any other bluetooth device on your cellphone to talk when making calls. This ‘Line #5, bluetooth linking’ is just a fancy feature of the SPA-525 to enable you to make cellphone calls, via your SPA-525"]

{"sheet":"2 - SPA525G Speed Dials","index":1,"n_rows":19,"n_cols":234,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Cisco SPA525G Main Lines"]
[]
["Line #","HH #","Name"]
["Line 2",301,"Public 1","fnc=sd;ext=301@$PROXY;nme=Public 1",{"$nulls":229},"fnc=sd;ext=301@$PROXY;nme=Public 1"]
["Line 3",302,"Public 2","fnc=sd;ext=302@$PROXY;nme=Public 2",{"$nulls":229},"fnc=sd;ext=302@$PROXY;nme=Public 2"]
["Line 4",303,"Public 3","fnc=sd;ext=303@$PROXY;nme=Public 3",{"$nulls":229},"fnc=sd;ext=303@$PROXY;nme=Public 3"]
["Line 5",336,"Gathering Spot.","fnc=sd;ext=336@$PROXY;nme=Gathering Spot.",{"$nulls":229},"fnc=sd;ext=336@$PROXY;nme=Gathering Spot."]
[]
["Instructions:"]
[]
["Enter HH# and Name (Do not change Line 5 if you have your cell phone linked to phone via Bluetooth)"]
[]
[]
[]
["Log into your SPA525G web interface as administrator/advanced user (http://xxx.xxx.xxx.xxx/admin/advanced)"]
[]
["Click Voice then Phone on the top tabs of your web interface, you will now see the Extended Functions for line key 2-5"]
[]
["Copy (Ctrl-C) the Purple Text and Paste (Ctrl-V) into the web interface Extended Functions for line key 2-5"]

{"sheet":"3 - Sidecar SPA500S","index":2,"n_rows":45,"n_cols":56,"rows_kept":45,"cut":false,"hidden":false,"merged":[[0,3,1,3],[0,4,1,4],[2,3,3,3],[2,4,3,4],[4,3,5,3],[4,4,5,4],[6,3,7,3],[6,4,7,4],[8,3,9,3],[8,4,9,4],[10,3,11,3],[10,4,11,4],[12,3,13,3],[12,4,13,4],[14,3,15,3],[14,4,15,4],[16,3,17,3],[16,4,17,4],[18,3,19,3],[18,4,19,4],[20,3,21,3],[20,4,21,4],[22,3,23,3],[22,4,23,4],[24,3,25,3],[24,4,25,4],[26,3,27,3],[26,4,27,4],[28,3,29,3],[28,4,29,4],[30,3,31,3],[30,4,31,4],[36,0,36,7],[37,0,37,7],[38,0,38,7],[39,0,39,7],[41,0,41,7],[42,0,42,7],[43,0,43,7],[44,0,44,7]],"flags":["formulas_cached_only"]}
[301,17,null,0,0,null,1,"fnc=sd;ext=301@$PROXY;nme=Public 1",{"$nulls":47},"fnc=sd;ext=301@$PROXY;nme=Public 1"]
["Public 1"," ",{"$nulls":4},2,"fnc=sd;ext=302@$PROXY;nme=Public 2",{"$nulls":47},"fnc=sd;ext=302@$PROXY;nme=Public 2"]
[302,18,null,0,0,null,3,"fnc=sd;ext=311@$PROXY;nme=HH INFO",{"$nulls":47},"fnc=sd;ext=311@$PROXY;nme=HH INFO"]
["Public 2"," ",{"$nulls":4},4,"fnc=sd;ext=4@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=4@$PROXY;nme= "]
[311,19,null,0,0,null,5,"fnc=sd;ext=5@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=5@$PROXY;nme= "]
["HH INFO"," ",{"$nulls":4},6,"fnc=sd;ext=6@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=6@$PROXY;nme= "]
[4,20,null,0,0,null,7,"fnc=sd;ext=7@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=7@$PROXY;nme= "]
[" "," ",{"$nulls":4},8,"fnc=sd;ext=8@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=8@$PROXY;nme= "]
[5,21,null,0,0,null,9,"fnc=sd;ext=9@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=9@$PROXY;nme= "]
[" "," ",{"$nulls":4},10,"fnc=sd;ext=10@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=10@$PROXY;nme= "]
[6,22,null,0,0,null,11,"fnc=sd;ext=11@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=11@$PROXY;nme= "]
[" "," ",{"$nulls":4},12,"fnc=sd;ext=12@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=12@$PROXY;nme= "]
[7,23,null,0,0,null,13,"fnc=sd;ext=13@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=13@$PROXY;nme= "]
[" "," ",{"$nulls":4},14,"fnc=sd;ext=14@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=14@$PROXY;nme= "]
[8,24,null,0,0,null,15,"fnc=sd;ext=15@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=15@$PROXY;nme= "]
[" "," ",{"$nulls":4},16,"fnc=sd;ext=16@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=16@$PROXY;nme= "]
[9,25,null,0,0,null,17,"fnc=sd;ext=17@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=17@$PROXY;nme= "]
[" "," ",{"$nulls":4},18,"fnc=sd;ext=18@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=18@$PROXY;nme= "]
[10,26,null,0,0,null,19,"fnc=sd;ext=19@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=19@$PROXY;nme= "]
[" "," ",{"$nulls":4},20,"fnc=sd;ext=20@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=20@$PROXY;nme= "]
[11,27,null,0,0,null,21,"fnc=sd;ext=21@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=21@$PROXY;nme= "]
[" "," ",{"$nulls":4},22,"fnc=sd;ext=22@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=22@$PROXY;nme= "]
[12,28,null,0,0,null,23,"fnc=sd;ext=23@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=23@$PROXY;nme= "]
[" "," ",{"$nulls":4},24,"fnc=sd;ext=24@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=24@$PROXY;nme= "]
[13,29,null,0,0,null,25,"fnc=sd;ext=25@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=25@$PROXY;nme= "]
[" "," ",{"$nulls":4},26,"fnc=sd;ext=26@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=26@$PROXY;nme= "]
[14,30,null,0,0,null,27,"fnc=sd;ext=27@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=27@$PROXY;nme= "]
[" "," ",{"$nulls":4},28,"fnc=sd;ext=28@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=28@$PROXY;nme= "]
[15,31,null,0,0,null,29,"fnc=sd;ext=29@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=29@$PROXY;nme= "]
[" "," ",{"$nulls":4},30,"fnc=sd;ext=30@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=30@$PROXY;nme= "]
[16,32,null,0,0,null,31,"fnc=sd;ext=31@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=31@$PROXY;nme= "]
[" "," ",{"$nulls":4},32,"fnc=sd;ext=32@$PROXY;nme= ",{"$nulls":47},"fnc=sd;ext=32@$PROXY;nme= "]
[]
[]
[]
[]
["Instructions:"]
[0]
["Fill in your data in columns A & B that you want to appear on your SPA500S sidecar."]
[0]
["Click this button"]
[0]
["Now you can copy the data in column H one at a time to your phones web interface (Advanced > ATT Console)"]
[]
["Then Print this page to create your sidecar label"]

{"sheet":"4 - Dial Outside Line","index":3,"n_rows":7,"n_cols":55,"rows_kept":7,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["If you set up your cell phone via bluetooth to line 5, then this conversion will allow you to dial to an outside number with line 5"]
["then this conversion will allow you to dial to an outside number with line 5"]
[]
["Phone Number:","3023327092"]
["Name:","HRO Delaware"]
[null,"fnc=sd;ext=3023327092@;vid=5;nme=HRO Delaware"]
[{"$nulls":54},0]